From 05044b9e4e4ae03f66e1c504d6fef57a1d135897 Mon Sep 17 00:00:00 2001
From: Dylan Van Assche <me@dylanvanassche.be>
Date: Thu, 24 Dec 2020 19:57:12 +0100
Subject: [PATCH] dts: pinephone: Add 'pine64,pinephone' to compat list

Indicates that all PinePhone models share most of the hardware with each other.
Used for feedbackd configuration when retrieving a device specific config for
haptic feedbackd.
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.0.dts | 2 +-
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts | 2 +-
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2.dts | 2 +-
 3 files changed, 3 insertions(+), 3 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.0.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.0.dts
index 0f6faa44c..2e0892b32 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.0.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.0.dts
@@ -7,7 +7,7 @@
 
 / {
 	model = "Pine64 PinePhone Developer Batch (1.0)";
-	compatible = "pine64,pinephone-1.0", "allwinner,sun50i-a64";
+	compatible = "pine64,pinephone-1.0", "pine64,pinephone", "allwinner,sun50i-a64";
 
 	reg_vbus: usb0-vbus {
 		compatible = "regulator-fixed";
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
index 95a880fdc..d6bad0838 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
@@ -7,7 +7,7 @@
 
 / {
 	model = "Pine64 PinePhone Braveheart (1.1)";
-	compatible = "pine64,pinephone-1.1", "allwinner,sun50i-a64";
+	compatible = "pine64,pinephone-1.1", "pine64,pinephone", "allwinner,sun50i-a64";
 
 	reg_vbus: usb0-vbus {
 		compatible = "regulator-fixed";
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2.dts
index 23ba72508..710493186 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2.dts
@@ -7,7 +7,7 @@
 
 / {
 	model = "Pine64 PinePhone (1.2)";
-	compatible = "pine64,pinephone-1.2", "allwinner,sun50i-a64";
+	compatible = "pine64,pinephone-1.2", "pine64,pinephone", "allwinner,sun50i-a64";
 
 	wifi_pwrseq: wifi-pwrseq {
 		compatible = "mmc-pwrseq-simple";
-- 
2.26.2

