From c4d3ac73a3f19d2372e3d35e833665b2ee1f11fa Mon Sep 17 00:00:00 2001
From: Martijn Braam <martijn@brixit.nl>
Date: Sat, 12 Dec 2020 13:31:03 +0100
Subject: [PATCH 1/8] PPP

---
 arch/arm/mach-rockchip/rk3399/Kconfig         |  7 ++
 board/pine64/pinephone-pro-rk3399/Kconfig     | 15 +++
 board/pine64/pinephone-pro-rk3399/MAINTAINERS |  8 ++
 board/pine64/pinephone-pro-rk3399/Makefile    |  1 +
 .../pinephone-pro-rk3399.c                    | 56 +++++++++++
 configs/pinephone-pro-rk3399_defconfig        | 92 +++++++++++++++++++
 6 files changed, 179 insertions(+)
 create mode 100644 board/pine64/pinephone-pro-rk3399/Kconfig
 create mode 100644 board/pine64/pinephone-pro-rk3399/MAINTAINERS
 create mode 100644 board/pine64/pinephone-pro-rk3399/Makefile
 create mode 100644 board/pine64/pinephone-pro-rk3399/pinephone-pro-rk3399.c
 create mode 100644 configs/pinephone-pro-rk3399_defconfig

diff --git a/arch/arm/mach-rockchip/rk3399/Kconfig b/arch/arm/mach-rockchip/rk3399/Kconfig
index 17628f9171..35b1125906 100644
--- a/arch/arm/mach-rockchip/rk3399/Kconfig
+++ b/arch/arm/mach-rockchip/rk3399/Kconfig
@@ -28,6 +28,13 @@ config TARGET_PINEBOOK_PRO_RK3399
 	  with 4Gb RAM, onboard eMMC, USB-C, a USB3 and USB2 port,
 	  1920*1080 screen and all the usual laptop features.
 
+config TARGET_PINEPHONE_PRO_RK3399
+	bool "PinePhone Pro"
+	help
+	  PinePhone Pro is a phone based on the Rockchip rk3399 SoC
+	  with 4Gb RAM, onboard eMMC, USB-C, a headphone jack,
+	  720x1440 screen and an external Quectel USB modem.
+
 config TARGET_PUMA_RK3399
 	bool "Theobroma Systems RK3399-Q7 (Puma)"
 	help
diff --git a/board/pine64/pinephone-pro-rk3399/Kconfig b/board/pine64/pinephone-pro-rk3399/Kconfig
new file mode 100644
index 0000000000..13d6465ae6
--- /dev/null
+++ b/board/pine64/pinephone-pro-rk3399/Kconfig
@@ -0,0 +1,15 @@
+if TARGET_PINEPHONE_PRO_RK3399
+
+config SYS_BOARD
+	default "pinephone-pro-rk3399"
+
+config SYS_VENDOR
+	default "pine64"
+
+config SYS_CONFIG_NAME
+	default "pinephone-pro-rk3399"
+
+config BOARD_SPECIFIC_OPTIONS
+	def_bool y
+
+endif
diff --git a/board/pine64/pinephone-pro-rk3399/MAINTAINERS b/board/pine64/pinephone-pro-rk3399/MAINTAINERS
new file mode 100644
index 0000000000..227c1c0bea
--- /dev/null
+++ b/board/pine64/pinephone-pro-rk3399/MAINTAINERS
@@ -0,0 +1,8 @@
+PINEBOOK_PRO
+M:	Peter Robinson <pbrobinson@gmail.com>
+S:	Maintained
+F:	board/pine64/rk3399-pinebook-pro/
+F:	include/configs/rk3399-pinebook-pro.h
+F:	arch/arm/dts/rk3399-pinebook-pro.dts
+F:	arch/arm/dts/rk3399-pinebook-pro-u-boot.dtsi
+F:	configs/pinebook-pro-rk3399_defconfig
diff --git a/board/pine64/pinephone-pro-rk3399/Makefile b/board/pine64/pinephone-pro-rk3399/Makefile
new file mode 100644
index 0000000000..8d9203053e
--- /dev/null
+++ b/board/pine64/pinephone-pro-rk3399/Makefile
@@ -0,0 +1 @@
+obj-y	+= pinephone-pro-rk3399.o
diff --git a/board/pine64/pinephone-pro-rk3399/pinephone-pro-rk3399.c b/board/pine64/pinephone-pro-rk3399/pinephone-pro-rk3399.c
new file mode 100644
index 0000000000..d79084614f
--- /dev/null
+++ b/board/pine64/pinephone-pro-rk3399/pinephone-pro-rk3399.c
@@ -0,0 +1,56 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * (C) Copyright 2019 Vasily Khoruzhick <anarsoul@gmail.com>
+ */
+
+#include <common.h>
+#include <dm.h>
+#include <init.h>
+#include <syscon.h>
+#include <asm/io.h>
+#include <asm/arch-rockchip/clock.h>
+#include <asm/arch-rockchip/grf_rk3399.h>
+#include <asm/arch-rockchip/hardware.h>
+#include <asm/arch-rockchip/misc.h>
+
+#define GRF_IO_VSEL_BT565_SHIFT 0
+#define PMUGRF_CON0_VSEL_SHIFT 8
+
+#ifdef CONFIG_MISC_INIT_R
+static void setup_iodomain(void)
+{
+	struct rk3399_grf_regs *grf =
+	    syscon_get_first_range(ROCKCHIP_SYSCON_GRF);
+	struct rk3399_pmugrf_regs *pmugrf =
+	    syscon_get_first_range(ROCKCHIP_SYSCON_PMUGRF);
+
+	/* BT565 is in 1.8v domain */
+	rk_setreg(&grf->io_vsel, 1 << GRF_IO_VSEL_BT565_SHIFT);
+
+	/* Set GPIO1 1.8v/3.0v source select to PMU1830_VOL */
+	rk_setreg(&pmugrf->soc_con0, 1 << PMUGRF_CON0_VSEL_SHIFT);
+}
+
+int misc_init_r(void)
+{
+	const u32 cpuid_offset = 0x7;
+	const u32 cpuid_length = 0x10;
+	u8 cpuid[cpuid_length];
+	int ret;
+
+	setup_iodomain();
+
+	ret = rockchip_cpuid_from_efuse(cpuid_offset, cpuid_length, cpuid);
+	if (ret)
+		return ret;
+
+	ret = rockchip_cpuid_set(cpuid, cpuid_length);
+	if (ret)
+		return ret;
+
+	ret = rockchip_setup_macaddr();
+
+	return ret;
+}
+
+#endif
diff --git a/configs/pinephone-pro-rk3399_defconfig b/configs/pinephone-pro-rk3399_defconfig
new file mode 100644
index 0000000000..320ce65ffb
--- /dev/null
+++ b/configs/pinephone-pro-rk3399_defconfig
@@ -0,0 +1,92 @@
+CONFIG_ARM=y
+CONFIG_ARCH_ROCKCHIP=y
+CONFIG_SYS_TEXT_BASE=0x00200000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_ENV_SIZE=0x8000
+CONFIG_ROCKCHIP_RK3399=y
+CONFIG_TARGET_PINEPHONE_PRO_RK3399=y
+CONFIG_DEBUG_UART_BASE=0xFF1A0000
+CONFIG_DEBUG_UART_CLOCK=24000000
+CONFIG_SPL_SPI_FLASH_SUPPORT=y
+CONFIG_SPL_SPI_SUPPORT=y
+CONFIG_DEFAULT_DEVICE_TREE="rk3399-pinephone-pro"
+CONFIG_DEBUG_UART=y
+CONFIG_BOOTDELAY=3
+CONFIG_USE_PREBOOT=y
+CONFIG_DEFAULT_FDT_FILE="rockchip/rk3399-pinephone-pro.dtb"
+CONFIG_DISPLAY_BOARDINFO_LATE=y
+CONFIG_MISC_INIT_R=y
+# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
+CONFIG_SPL_STACK_R=y
+CONFIG_SPL_STACK_R_MALLOC_SIMPLE_LEN=0x10000
+CONFIG_SPL_MTD_SUPPORT=y
+CONFIG_SPL_SPI_LOAD=y
+CONFIG_TPL=y
+CONFIG_CMD_BOOTZ=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_I2C=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_PCI=y
+CONFIG_CMD_USB=y
+# CONFIG_CMD_SETEXPR is not set
+CONFIG_CMD_TIME=y
+CONFIG_CMD_PMIC=y
+CONFIG_CMD_REGULATOR=y
+CONFIG_SPL_OF_CONTROL=y
+CONFIG_OF_SPL_REMOVE_PROPS="pinctrl-0 pinctrl-names clock-names interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
+CONFIG_ENV_IS_IN_SPI_FLASH=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_ROCKCHIP_GPIO=y
+CONFIG_SYS_I2C_ROCKCHIP=y
+CONFIG_DM_KEYBOARD=y
+CONFIG_LED=y
+CONFIG_LED_GPIO=y
+CONFIG_MISC=y
+CONFIG_ROCKCHIP_EFUSE=y
+CONFIG_MMC_DW=y
+CONFIG_MMC_DW_ROCKCHIP=y
+CONFIG_MMC_SDHCI=y
+CONFIG_MMC_SDHCI_SDMA=y
+CONFIG_MMC_SDHCI_ROCKCHIP=y
+CONFIG_SF_DEFAULT_SPEED=20000000
+CONFIG_SPI_FLASH_GIGADEVICE=y
+CONFIG_SPI_FLASH_WINBOND=y
+CONFIG_DM_ETH=y
+CONFIG_NVME=y
+CONFIG_PCI=y
+CONFIG_PHY_ROCKCHIP_INNO_USB2=y
+CONFIG_PHY_ROCKCHIP_TYPEC=y
+CONFIG_DM_PMIC_FAN53555=y
+CONFIG_PMIC_RK8XX=y
+CONFIG_REGULATOR_PWM=y
+CONFIG_REGULATOR_RK8XX=y
+CONFIG_PWM_ROCKCHIP=y
+CONFIG_RAM_RK3399_LPDDR4=y
+CONFIG_DM_RESET=y
+CONFIG_DM_RNG=y
+CONFIG_RNG_ROCKCHIP=y
+CONFIG_BAUDRATE=1500000
+CONFIG_DEBUG_UART_SHIFT=2
+CONFIG_ROCKCHIP_SPI=y
+CONFIG_SYSRESET=y
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_DWC3=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_EHCI_GENERIC=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_OHCI_GENERIC=y
+CONFIG_USB_DWC3=y
+CONFIG_USB_DWC3_GENERIC=y
+CONFIG_USB_KEYBOARD=y
+CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
+CONFIG_USB_HOST_ETHER=y
+CONFIG_USB_ETHER_ASIX=y
+CONFIG_USB_ETHER_RTL8152=y
+CONFIG_DM_VIDEO=y
+CONFIG_DISPLAY=y
+CONFIG_VIDEO_ROCKCHIP=y
+CONFIG_DISPLAY_ROCKCHIP_EDP=y
+CONFIG_SPL_TINY_MEMSET=y
+CONFIG_ERRNO_STR=y
-- 
2.33.0
