From e8be2e4affb906af7137437ac62fb3912609c11e Mon Sep 17 00:00:00 2001
From: Ondrej Jirman
Date: Thu, 29 Oct 2020 04:55:40 +0100
Subject: drm: panel: st7703: Fix xbd599 timings to make refresh rate exactly
 60.006Hz

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/gpu/drm/panel/panel-sitronix-st7703.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

diff --git a/drivers/gpu/drm/panel/panel-sitronix-st7703.c b/drivers/gpu/drm/panel/panel-sitronix-st7703.c
index 4287aabb9007..070ef2baef6f 100644
--- a/drivers/gpu/drm/panel/panel-sitronix-st7703.c
+++ b/drivers/gpu/drm/panel/panel-sitronix-st7703.c
@@ -334,14 +334,14 @@ static int xbd599_init_sequence(struct st7703 *ctx)
 
 static const struct drm_display_mode xbd599_mode = {
 	.hdisplay    = 720,
-	.hsync_start = 720 + 40,
-	.hsync_end   = 720 + 40 + 40,
-	.htotal	     = 720 + 40 + 40 + 40,
+	.hsync_start = 720 + 30,
+	.hsync_end   = 720 + 30 + 28,
+	.htotal	     = 720 + 30 + 28 + 30,
 	.vdisplay    = 1440,
 	.vsync_start = 1440 + 18,
 	.vsync_end   = 1440 + 18 + 10,
 	.vtotal	     = 1440 + 18 + 10 + 17,
-	.clock	     = 69000,
+	.clock	     = 72000,
 	.flags	     = DRM_MODE_FLAG_NHSYNC | DRM_MODE_FLAG_NVSYNC,
 	.width_mm    = 68,
 	.height_mm   = 136,
-- 
cgit v1.2.3

