From 7045054c96224ead00aae09246f475dfe6202def Mon Sep 17 00:00:00 2001
From: Danct12 <danct12@disroot.org>
Date: Tue, 19 Jan 2021 10:09:01 +0700
Subject: [PATCH] arm64: dts: allwinner: pinephone: stop LEDs on suspend

Signed-off-by: Danct12 <danct12@disroot.org>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 3 ---
 1 file changed, 3 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index 02d82980c..00ed866ae 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -218,14 +218,12 @@
 			function = LED_FUNCTION_INDICATOR;
 			color = <LED_COLOR_ID_BLUE>;
 			gpios = <&pio 3 20 GPIO_ACTIVE_HIGH>; /* PD20 */
-			retain-state-suspended;
 		};
 
 		green {
 			function = LED_FUNCTION_INDICATOR;
 			color = <LED_COLOR_ID_GREEN>;
 			gpios = <&pio 3 18 GPIO_ACTIVE_HIGH>; /* PD18 */
-			retain-state-suspended;
 		};
 
 		red {
@@ -233,7 +231,6 @@
 			function = LED_FUNCTION_INDICATOR;
 			color = <LED_COLOR_ID_RED>;
 			gpios = <&pio 3 19 GPIO_ACTIVE_HIGH>; /* PD19 */
-			retain-state-suspended;
 		};
 	};
 
-- 
2.30.0

