From 7dd3866d9c2bef4bb73a781861aeeec595510509 Mon Sep 17 00:00:00 2001
From: Arnaud Ferraris <arnaud.ferraris@collabora.com>
Date: Fri, 3 Apr 2020 17:13:55 +0200
Subject: [PATCH] arm64: dts: allwinner: pinetab: enable jack detection

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
index a87790df9..a72c2ec8c 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
@@ -117,11 +117,13 @@ wifi_pwrseq: wifi_pwrseq {
 };
 
 &codec {
+	allwinner,inverted-jack-detection;
 	status = "okay";
 };
 
 &codec_analog {
 	cpvdd-supply = <&reg_eldo1>;
+	allwinner,internal-bias-resistor;
 	status = "okay";
 };
 
@@ -448,6 +450,7 @@ &reg_rtc_ldo {
 
 &sound {
 	status = "okay";
+	simple-audio-card,name = "PineTab";
 	simple-audio-card,aux-devs = <&codec_analog>, <&speaker_amp>;
 	simple-audio-card,widgets = "Microphone", "Internal Microphone Left",
 				    "Microphone", "Internal Microphone Right",
-- 
2.28.0

