From 13c8c6945856e57958fdf7e4ef338c21e1199f19 Mon Sep 17 00:00:00 2001
From: Martijn Braam <martijn@brixit.nl>
Date: Sun, 13 Dec 2020 19:52:09 +0100
Subject: [PATCH 5/8] Add pinephone-pro-rk3399.h

---
 include/configs/pinephone-pro-rk3399.h | 22 ++++++++++++++++++++++
 1 file changed, 22 insertions(+)
 create mode 100644 include/configs/pinephone-pro-rk3399.h

diff --git a/include/configs/pinephone-pro-rk3399.h b/include/configs/pinephone-pro-rk3399.h
new file mode 100644
index 0000000000..aaaa344839
--- /dev/null
+++ b/include/configs/pinephone-pro-rk3399.h
@@ -0,0 +1,22 @@
+/* SPDX-License-Identifier: GPL-2.0+ */
+/*
+ * Copyright (C) 2016 Rockchip Electronics Co., Ltd
+ * Copyright (C) 2020 Peter Robinson <pbrobinson at gmail.com>
+ */
+
+#ifndef __PINEPHONE_PRO_RK3399_H
+#define __PINEPHONE_PRO_RK3399_H
+
+#define ROCKCHIP_DEVICE_SETTINGS \
+		"stdin=serial,usbkbd\0" \
+		"stdout=serial,vidconsole\0" \
+		"stderr=serial,vidconsole\0"
+
+#include <configs/rk3399_common.h>
+
+#define SDRAM_BANK_SIZE			(2UL << 30)
+
+#define CONFIG_USB_OHCI_NEW
+#define CONFIG_SYS_USB_OHCI_MAX_ROOT_PORTS     2
+
+#endif
-- 
2.33.0

